Audio loop back cable |

(Applicable to BurnInTest Pro version only)
|  | PassMark audio loopback cables contain two 3.5mm gold plated stereo plugs which connect the Audio out and microphone in ports of your sound card during sound card loopback testing.
The following are the cable specifications. Dimensions: Total length: 330mm ± 0.5mm Plug length: 14mm ± 0.5mm Plug diameter: 3.5mm Conductors: American wiring gauge: (26(10/0.12)x2F, 0.43mm diameter Insulation: PBC, 1.0mm diameter Shielding: Spiral shield: Bare copper wire, 30/0.10 Sheath: Material: PVC Color: Black Audio loopback cables can be purchased from http://www.passmark.com