Temperature |

This part of the main window displays the temperature of hardware the components configured for temperaure monitoring during testing. Temperature display The minimum, current and maximum temperature of up to 6 hardware components is displayed. The temperature scale, Celcius or Farenheight, and the temperature sources are selected in Prefernces->Temp / Battery. See Test preferences - Temperature. Temperatures are updated during testing; after a test is complete the temperatures shown will be for the previous test run. A color key shows which hardware is represented by a temperature timeline in the graph below. Temperature graph The temperature graph shows each of the temperature sources graphed over time. There are 2 lines of the same color shown for each temperature source, (1) a thicker line shows the temperature for the hardware selected and (2) a thinner line shows the temperature threshold for that hardware. One temperature line may obscure other temperature lines. The X-axis is time, and the Y-axis temperature. Up to the last 1000 temperature samples are stored during a test. The time axis is scaled based on the temperature sample duration (set in preferences). The temperature axis is scaled based on the temperature values and temperature thresholds.