Example text log file |

PassMark BurnInTest Log file - http://www.passmark.com ======================================================== Date: 01/20/14 13:34:48 BurnInTest V8.0 Pro 0000 (64-bit) Customer: HP Technician: Ian Machine type: Passmark123 Machine serial #: 12345-ABC Notes: Additional notes System summary: Windows 7 Ultimate Edition Service Pack 1 build 7601 (64-bit), 1 x Intel(R) Core(TM) i5-2500K CPU @ 3.30GHz [2007.2 MHz], 8.0GB RAM, AMD Radeon HD 6790, 932GB HDD, 112GB SSD, CD-RW/DVDRW, General: System Name: PASSMARKI2500K0 Motherboard Manufacturer: ASUSTeK Computer INC. Motherboard Name: P8Z68-V PRO Motherboard Version: Rev 1.xx Motherboard Serial Number: 109822190000539 BIOS Manufacturer: American Megatrends Inc. BIOS Version: 0401 BIOS Release Date: 04/29/2011 CPU: CPU manufacturer: GenuineIntel CPU Type: Intel(R) Core(TM) i5-2500K CPU @ 3.30GHz Codename: Sandy Bridge CPUID: Family 6, Model 2A, Stepping 7, Revision D2 Socket: LGA1155 Lithography: 32nm Physical CPU's: 1 Cores per CPU: 4 Hyperthreading: Disabled CPU features: MMX SSE SSE2 SSE3 SSSE3 SSE4.1 SSE4.2 DEP PAE Intel64 VMX Turbo AES AVX FMA3 Clock frequencies: - Measured CPU speed: 2007.2 MHz [Turbo: 3613.0MHz] - Multiplier: x20.0 [Turbo: x36.0] - Base Clock: 100.0 MHz Multiplier range: Min: x16, Max non turbo: x20 [Turbo: 4C: x34, 3C: x35, 2C: x36, 1C: x37] Cache per CPU package: - L1 Instruction Cache: 4 x 32 KB - L1 data cache: 4 x 32 KB - L2 cache: 4 x 256 KB - L3 cache: 6 MB Memory Total Physical Memory: 8169MB Available Physical Memory: 4182MB Memory devices: Slot 1: - 4GB DDR3 SDRAM PC3-12800 - Corsair CMZ8GX3M2A1600C9 - XMP: 1.50V, Clk: 800.0MHz, Timings 9-9-9-24 Slot 2: - 4GB DDR3 SDRAM PC3-12800 - Corsair CMZ8GX3M2A1600C9 - XMP: 1.50V, Clk: 800.0MHz, Timings 9-9-9-24 Slot 3: - Not populated Slot 4: - Not populated Virtual memory: C:\pagefile.sys (allocated base size 500MB) Graphics AMD Radeon HD 6790 Chip Type: ATI display adapter (0x673E) DAC Type: Internal DAC(400MHz) Memory: 1024MB BIOS: 113-3E17420-S4A Driver provider: Advanced Micro Devices, Inc. Driver version: 8.950.0.0 Driver date: 2-14-2012 Monitor 1: 1680x1050x32 60Hz (Primary monitor) Disk volumes C: Local Drive, NTFS, (111.69GB total, 8.26GB free) D: Local Drive, New Volume, NTFS, (911.98GB total, 184.26GB free) E: Local Drive, New Volume, NTFS, (0.98GB total, 0.00GB free) F: Local Drive, New Volume, NTFS, (0.98GB total, 0.47GB free) G: Optical drive, PASSMARK_DVD, UDF H: Local Drive, NEW VOLUME, FAT32, (0.09GB total, 0.09GB free) I: Local Drive, NEW VOLUME, FAT32, (0.09GB total, 0.09GB free) J: Local Drive, NEW VOLUME, FAT, (0.10GB total, 0.01GB free) L: Local Drive, New Volume, NTFS, (0.98GB total, 0.94GB free) Disk drives Disk drive: Model: ST31000524AS ATA Device Serial: 6VPBZ614 (Disk: 0, Size: 931.51GB, Volumes: D E F H I J L) Disk drive: Model: OCZ-VERT EX3 SCSI Disk Device Serial: OCZ-374X01L7M4293C45 (Disk: 1, Size: 111.79GB, Volumes: C) Optical drives G: HL-DT-ST DVDRAM GH22NS70 (CD-RW/DVDRW) Network Intel(R) 82579V Gigabit Network Connection (Speed: 100Mb/s) (MAC: F4:6D:04:3D:88:C6) ASUS NX1101 Gigabit Ethernet Adapter (MAC: 00:22:15:10:8D:35) Ports Keyboard Port: PS/2 connector USB Intel(R) 6 Series/C200 Series Chipset Family USB Enhanced Host Controller - 1C2D - (SN: BC7B0683) Intel(R) 6 Series/C200 Series Chipset Family USB Enhanced Host Controller - 1C26 - Microsoft Natural Ergonomic Keyboard 4000 - PASSMARK USB2Test (SN: PMPOHEVN) - USB Input Device ASMedia XHCI Controller - PassMark USB3Test (SN: PMYK8IPL) ASMedia XHCI Controller ****************** DETAILED EVENT LOG ****************** LOG NOTE: 2014-01-20 13:37:35, Status, Webcam pre-test started LOG NOTE: 2014-01-20 13:37:38, Status, Microphone pre-test started LOG NOTE: 2014-01-20 13:37:40, Microphone, Microphone test passed LOG NOTE: 2014-01-20 13:37:41, Status, Main Tests started LOG NOTE: 2014-01-20 13:37:42, CPU, SSE4a test(s) selected, but CPU feature not detected LOG NOTE: 2014-01-20 13:37:42, 3D Graphics, 3D test starting: Duty cycle = 50. Test on primary monitor (0). (x,y) = (200,-18). WxH = 1280x1024. LOG NOTE: 2014-01-20 13:37:44, 3D Graphics, 3D test starting: Duty cycle = 50. Test on monitor number 1. (x,y) = (220,2). WxH = 1280x1024. LOG NOTE: 2014-01-20 13:37:45, 3D Graphics, 3D test starting: Duty cycle = 50. Test on monitor number 2. (x,y) = (240,22). WxH = 1280x1024. LOG NOTE: 2014-01-20 13:37:47, 3D Graphics, 3D test starting: Duty cycle = 50. Test on monitor number 3. (x,y) = (260,42). WxH = 1280x1024. LOG NOTE: 2014-01-20 13:37:50, Video, Video test starting: Duty cycle = 50. Test on primary monitor (0). (x,y) = (310,200). WxH = 300x200. LOG NOTE: 2014-01-20 13:38:42, Status, Test run stopped ************** RESULT SUMMARY ************** Test Start time: Mon Jan 20 13:37:40 2014 Test Stop time: Mon Jan 20 13:38:42 2014 Test Duration: 000h 01m 02s Temperature CPU 0 average (Min/Current/Max): 42.3C / 64.5C / 65.0C Temperature CPU 0 core 0 (Min/Current/Max): 41.0C / 64.0C / 64.0C Temperature CPU 0 core 1 (Min/Current/Max): 44.0C / 64.0C / 66.0C Temperature CPU 0 core 2 (Min/Current/Max): 39.0C / 63.0C / 63.0C Temperature CPU 0 core 3 (Min/Current/Max): 45.0C / 67.0C / 67.0C Temperature HDD 0 (ST31000524AS ATA Device) (Min/Current/Max): 29.0C / 29.0C / 29.0C Temperature GPU 0 (AMD Radeon HD 6700 Series) (Min/Current/Max): 55.0C / 67.0C / 67.0C Test Name Cycles Operations Result Errors Last Error CPU 3 42.188 Billion PASS 0 No errors Memory (RAM) 1 3.778 Billion PASS 0 No errors 2D Graphics 0 255 PASS 0 No errors 3D Graphics 0 2729 PASS 0 No errors Temperature - - PASS 0 No errors Optical disk (G:) 1 167 Million PASS 0 No errors USB 3 (PMYK8IPL 5Gb/s) 0 2.840 Billion PASS 0 No errors USB 2 (PMPOHEVN 480Mb/s) 0 19.698 Million PASS 0 No errors Sound 0 970200 PASS 0 No errors Video Playback 1 30 PASS 0 No errors Webcam 0 15.974 Million PASS 0 No errors Microphone 1 1 PASS 0 No errors Disk (C:) 3 7.726 Billion PASS 0 No errors Network 1 0 7680 PASS 0 No errors TEST RUN PASSED ******************************************* SERIOUS ERROR SUMMARY FOR THE LAST TEST RUN ******************************************* ----------------------------------------------------------------------------------------------------- Note: Text files are stored in UNICODE (not ASCII) which allows for the consistent encoding, representation and handling of text expressed in most of the world's writing systems. See also Detailed error log Test preferences - Logging