## BurnInTest results

BurnInTest Version | V8.0 Pro 1040
Date | Wed Apr 29 16:24:50 2020
Logging level | Normal

## System summary

Windows 8.1 Professional Edition build 9600 (64-bit),
1 x Intel(R) Core(TM) i5-6400 CPU @ 2.70GHz,
7.9GB RAM,
Intel(R) HD Graphics 530,
56GB SSD, 119GB HDD,

### General

System Name: | HUCHANGHUI
System Model: | Default string
Motherboard Manufacturer: | Default string
Motherboard Name: | SKYBAY
Motherboard Version: | Default string
Motherboard Serial Number: | Default string
BIOS Manufacturer: | ALASKA - 1072009
BIOS Release Date: | 2017/11/30

### CPU

CPU manufacturer: | GenuineIntel
CPU Type: | Intel(R) Core(TM) i5-6400 CPU @ 2.70GHz
CPUID | Family 6, Model 5E, Stepping 3
Physical CPU's: | 1
Cores per CPU: | 4
Hyperthreading: | Disabled
CPU features: | MMX SSE SSE2 SSE3 SSSE3 SSE4.1 SSE4.2 DEP PAE Intel64 VMX AES AVX AVX2 XOP FMA3
Cache per CPU package: |
- L1 Instruction Cache: | 4 x 32 KB
- L1 data cache: | 4 x 32 KB
- L2 cache: | 4 x 256 KB
- L3 cache: | 6 MB

### Memory

Total Physical Memory: | 8112MB
Available Physical Memory: | 3504MB
Virtual memory: | C:\pagefile.sys (allocated base size 1280MB)

### Memory SPD

### Graphics

Intel(R) HD Graphics 530 |
Chip Type: | Intel(R) HD Graphics Family
DAC Type: | Internal
Memory: | 1024MB
BIOS: | Intel Video BIOS
Driver provider: | Intel Corporation
Driver version: | 26.20.100.7263
Driver date: | 9-25-2019
Monitor 1: | 2560x1080x32 50Hz (Primary monitor)

### Disk volumes

C: Local Drive, \\?\Volume{f475530c-76e3-4031-8e79-8acf8df5dfe4}\, NTFS, (118.08GB total, 75.51GB free)
D: Local Drive, \\?\Volume{67e2c54a-4038-476b-b8f5-fb3dd2a3f1d3}\, NTFS, (55.90GB total, 34.83GB free)
E: Local Drive, \\?\Volume{f2538f3e-0000-0000-0000-200000000000}\, NTFS, (465.76GB total, 172.17GB free)
F: Removable
G: Optical drive

### Disk drives

磁盘驱动器: Model: Kingston DataTraveler 3.0 USB Device Serial: N/A (Disk: 3, Size: 28.87GB, Volumes: N/A)
磁盘驱动器: Model: Generic External USB Device Serial: Z2A41ENY (Disk: 2, Size: 465.76GB, Volumes: E)
磁盘驱动器: Model: KINGSTON SV300S37A60G Serial: 50026B775304200F (Disk: 0, Size: 55.90GB, Volumes: D)
磁盘驱动器: Model: SAMSUNG MZVLW128HEGR-00000 Serial: N/A (Disk: 1, Size: 119.24GB, Volumes: C)

### Optical drives

### Network

Intel(R) I211 Gigabit Network Connection (Speed: 1Gb/s) (MAC: 40:62:31:00:77:47)
Intel(R) I211 Gigabit Network Connection (MAC: 40:62:31:00:77:46)

### Ports

通信端口: COM1 - RS232 Serial Port (max Baud rate: 115200)
通信端口: COM2 - RS232 Serial Port (max Baud rate: 115200)
通信端口: COM3 - RS232 Serial Port (max Baud rate: 115200)
通信端口: COM4 - RS232 Serial Port (max Baud rate: 115200)
Mouse Port: PS/2 connector
Keyboard Port: PS/2 connector

### USB

符合 USB xHCI 的主机控制器
- USB 输入设备
- Logitech Gaming Mouse G302 (SN: 0C6F37483430)
- Generic External (SN: 5A32413431454E5920202020)
- Kingston DataTraveler 3.0 (SN: 60A44C413DF8E2B1999A51D9)

## Detailed event log

Event
LOG NOTE: 2020-04-29 16:24:50, Status, PassMark BurnInTest V8.0 Pro 1040 (32-bit)
LOG NOTE: 2020-04-29 16:24:52, Status, Main Tests started
LOG NOTE: 2020-04-29 16:24:52, 3D Graphics, 3D test starting: Duty cycle = 100. Test on primary monitor (0). (x,y) = (1130,408). WxH = 300x200.
WARNING: 2020-04-29 16:24:58, 3D Graphics, The 3D test was interrupted
LOG NOTE: 2020-04-29 16:25:00, Status, Test run stopped

## Result summary

Test Start time | Wed Apr 29 16:24:50 2020
Test Stop time | Wed Apr 29 16:25:00 2020
Test Duration | 000h 00m 10s
Temperature HDD 0 (KINGSTON SV300S37A60G) (Min/Current/Max) | NA / NA / NA
Temperature HDD 2 (Generic External USB Device) (Min/Current/Max) | NA / NA / NA

Test | Cycles | Operations | Result | Errors | Last Error
3D Graphics | 0 | 135 | FAIL | 1 | The 3D test was interrupted
Temperature | - | - | PASS | 0 | No errors

TEST RUN FAILED

## Serious error summary for the last test run

Serious and critical errors
No serious or critical errors