#__________________________________________________________
#
# PassMark Software
# SysInfo 
# String Localizations
#__________________________________________________________
#
# Configuring String Localizations
#
# Each of the strings in SysInfo can be changed 
# to include a customer specific string or wording. 
# The file localization.txt (this file that stored in the 
# software directory) contains the strings used 
# by SysInfo. 
#
# The file is formatted as a Comma Separated File with two required fields:
#
# 1. STRING ID - this must not be changed by the customer; 
# 2. String text - this may be changed. This must be a 
#    string enclosed by quotes; 
#
#    a. Parameters must remain in their initially assigned order.
#       For example, in the string below:
#
#       "The file %s (%d Bytes) in folder %s could not be opened."
#
#       -file %s must be the first parameter
#       -%d bytes must be the second parameter
#       -folder %s must be the third parameter
#
# Additional comma separated values will be ignored and can be used for comments.
#
# IMPORTANT: A comma is required after the second field, even if you do not have additional comments.
#
# 3+. Customer comment – this is optional and may be changed – it is 
#     ignored by SysInfo. 
#
#
# Notes:
#   (i) SysInfo must be restarted after making changes to this file
#  (ii) You need to run SysInfo with sufficient privileges to save 
#       this file in the SysInfo directory.
# (iii) A comment is indicated by a "#" at the start of the line.
#  (iv) This file may be deleted on uninstalling SysInfo or installing
#       a new version of SysInfo. It is recommended that you keep a 
#       separate copy of this file.
#   (v) It is important that you keep the strings relatively the same length
#       after translating. Longer strings may be truncated by the available
#       space in the GUI. 
#  (vi) Maximum line length (including any comments) cannot exceed 1024 characters
#__________________________________________________________
#
# PassMark SysInfo,,, 
# Program String Text,,,
#
# Translation Notes:
# NOTE: SMART is Self-Monitoring, Analysis and Reporting Technology - the word does not need to be translated
# NOTE: LBA stands for Logical Block Addressing - the word does not need to be translated
# NOTE: Some other abbreviated words that do not need to be translated: HPA, DCO, SMTP, TEC
# NOTE: Use you best judgement when it comes to abbreviated words
#
#
# [General Strings]
SI_IDS_NA,"Not applicable",
SI_IDS_NA_ABV,"N/A",
SI_IDS_OTHER,"Other",
SI_IDS_READY,"Ready",
SI_IDS_UNKNOWN,"Unknown",
SI_IDS_NETWORKED,"Networked",
SI_IDS_NOT_CAPABLE,"Not capable",
SI_IDS_ENABLED,"Enabled",
SI_IDS_DISABLED,"Disabled",
SI_IDS_SUPPORTED,"Supported",
SI_IDS_NOT_SUPPORTED,"Not supported",
SI_IDS_SUPPORTED_NOT_ENABLED,"Supported, not enabled",
SI_IDS_MIN,"Min",
SI_IDS_MAX,"Max",
SI_IDS_KB,"KB",
SI_IDS_MB,"MB",
SI_IDS_GB,"GB",
SI_IDS_YES,"Yes",
SI_IDS_NO,"No",
SI_IDS_REGISTERED,"registered",
SI_IDS_NONE,"None",
SI_IDS_SERIAL,"Serial",
SI_IDS_PARALLEL,"Parallel",
#
#
# [General Error Strings]
SI_IDS_INVALID_HANDLE,"Invalid handle",
SI_IDS_INSUFFICIENT_MEM,"Insufficient memory",
SI_IDS_BUFFER_TOO_SMALL,"Data buffer too small",
SI_IDS_UNABLE_OPEN_DEVICE,"Unable to open device",
SI_IDS_ADMIN_REQUIRED,"Access denied. Administrator privilege required.",
SI_IDS_DRIVER_MISSING,"Error initializing device driver. Try re-installing the application.",
SI_IDS_DRIVER_VERSION,"Device driver version incompatible with this software. Try re-installing the application.",
SI_IDS_UNABLE_CPU_INFO,"Unable to obtain CPU information.",
SI_IDS_CREATE_FAIL,"Failed to create file.",
SI_IDS_OPEN_FAIL,"Failed to open file.",
#
#
# [System Info Strings]
SI_IDS_INTEL_COMPATIBLE,"Intel compatible",
SI_IDS_REMOVABLE,"Removable",
SI_IDS_RAMDISK,"RAMdisk",
SI_IDS_RAM,"RAM",
SI_IDS_CPU,"CPU",
SI_IDS_OPTICAL_DRIVE,"Optical drive",
SI_IDS_LOCAL_DRIVE,"Local Drive",
SI_IDS_FLOPPY,"Floppy",
SI_IDS_SYSTEM_SUMMARY,"System summary",
SI_IDS_GENERAL,"General",
SI_IDS_SYSTEM_NAME,"System Name:",
SI_IDS_SYSTEM_MODEL,"System Model:",
SI_IDS_MOTHERBOARD_MANUFACTURER,"Motherboard Manufacturer:",
SI_IDS_MOTHERBOARD_NAME,"Motherboard Name:",
SI_IDS_MOTHERBOARD_MODEL,"Motherboard Model:",
SI_IDS_MOTHERBOARD_VERSION,"Motherboard Version:",
SI_IDS_MOTHERBOARD_SERIAL_NUMBER,"Motherboard Serial Number:",
SI_IDS_BIOS_MANUFACTURER,"BIOS Manufacturer:",
SI_IDS_BIOS_VERSION,"BIOS Version:",
SI_IDS_BIOS_RELEASE_DATE,"BIOS Release Date:",
SI_IDS_MEASURED_CPU_SPEED,"Measured CPU speed",
SI_IDS_MULTIPLIER,"Multiplier",
SI_IDS_SCALABLE_BUS_SPEED,"Scalable Bus Speed",
SI_IDS_STOCK,"Stock",
SI_IDS_MHZ,"MHz",
SI_IDS_BASE_CLOCK,"Base Clock",
SI_IDS_REFERENCE_CLOCK,"Reference Clock",
SI_IDS_FRONT_SIDE_BUS,"Front Side Bus",
SI_IDS_NON_TURBO,"non turbo",
SI_IDS_MULIPLIER_RANGE,"Multiplier range",
SI_IDS_TRACE_CACHE,"Trace Cache",
SI_IDS_L1_INSTRUCTION_CACHE,"L1 Instruction Cache",
SI_IDS_CPU_MANUFACTURER,"CPU manufacturer:",
SI_IDS_CPU_TYPE,"CPU Type:",
SI_IDS_CODENAME,"Codename:",
SI_IDS_SOCKET,"Socket:",
SI_IDS_LITHOGRAPHY,"Lithography:",
SI_IDS_PHYSICAL_CPUS,"Physical CPU's:",
SI_IDS_CORES_PER_CPU,"Cores per CPU:",
SI_IDS_HYPERTHREADING,"Hyperthreading:",
SI_IDS_CPU_FEATURES,"CPU features:",
SI_IDS_CLOCK_FREQUENCIES,"Clock frequencies:",
SI_IDS_HT_LINK,"-  HT Link",
SI_IDS_CACHE_PER_CPU_PACKAGE,"Cache per CPU package:",
SI_IDS_DATA_CACHE,"Data Cache",
SI_IDS_CACHE,"Cache",
SI_IDS_TDP_LIMIT,"TDP Limit:",
SI_IDS_WATTS,"%d Watts",
SI_IDS_AMPS,"%d Amps",
SI_IDS_MANUFACTURER,"Manufacturer",
SI_IDS_SERIAL_NUMBER,"Serial#",
SI_IDS_NOT_POPULATED,"Not populated",
SI_IDS_MEMORY,"Memory",
SI_IDS_TOTAL_PHYSICAL_MEMORY,"Total Physical Memory:",
SI_IDS_AVAILABLE_PHYSICAL_MEMORY,"Available Physical Memory:",
SI_IDS_MEMORY_DEVICES,"Memory devices:",
SI_IDS_VIRTUAL_MEMORY,"Virtual memory:",
SI_IDS_ALLOCATED_BASE_SIZE,"allocated base size",
SI_IDS_GRAPHICS,"Graphics",
SI_IDS_CHIP_TYPE,"Chip Type:",
SI_IDS_DAC_TYPE,"DAC Type:",
SI_IDS_DRIVER_PROVIDER,"Driver provider:",
SI_IDS_DRIVER_VERSION2,"Driver version:",
SI_IDS_DRIVER_DATE,"Driver date:",
SI_IDS_DISK_VOLUMES,"Disk volumes",
SI_IDS_DISK_DRIVES,"Disk drives",
SI_IDS_OPTICAL_DRIVES,"Optical drives",
SI_IDS_NETWORK,"Network",
SI_IDS_PORTS,"Ports",
SI_IDS_MAX_BAUD_RATE,"max Baud rate",
SI_IDS_PARALLEL_PORT,"Parallel port:",
SI_IDS_CONNECTOR,"connector",
SI_IDS_USB_NOT_DETECTED,"USB not detected",
SI_IDS_L1_DATA_CACHE,"-  L1 data cache:",
SI_IDS_L2_CACHE,"-  L2 cache:",
SI_IDS_L3_CACHE,"-  L3 cache:",
SI_IDS_TDC_LIMIT,"TDC limit:",
SI_IDS_MEMORY_C,"Memory:",
SI_IDS_BIOS_C,"BIOS:",
SI_IDS_MEMSPD,"Memory SPD",
SI_IDS_MEM_TYPE,"Memory type:",
SI_IDS_MEM_SPDREV,"SPD revision:",
SI_IDS_MEM_MANUF,"Manufacturer:",
SI_IDS_MEM_MANUF_DATE,"Manufacturing date:",
SI_IDS_MEM_SERIALNO,"Serial number:",
SI_IDS_MEM_PARTNO,"Part number:",
SI_IDS_MEM_SPEED,"Clock speed:",
SI_IDS_MEM_SIZE,"Memory size:",
SI_IDS_MEM_BANKS,"Number of banks:",
SI_IDS_MEM_ROWS,"Row address bits:",
SI_IDS_MEM_COLS,"Column address bits:",
SI_IDS_MEM_BUSWIDTH,"Bus width:",
SI_IDS_MEM_DEVWIDTH,"Device width:",
SI_IDS_MEM_VOLTAGE,"Module voltage:",
SI_IDS_MEM_T_CK,"Minimum clock cycle time (tCK):",
SI_IDS_MEM_CAS_LAT,"Supported CAS latencies:",
SI_IDS_MEM_T_AA,"Minimum CAS latency time (tAA):",
SI_IDS_MEM_T_RCD,"Minimum RAS to CAS delay time (tRCD):",
SI_IDS_MEM_T_RP,"Minimum row precharge time (tRP):",
SI_IDS_MEM_T_RAS,"Minimum active to precharge time (tRAS):",
SI_IDS_MEM_TIMING,"Supported timing at highest clock speed:",
SI_IDS_MEM_T_RRD,"Minimum Row Active to Row Active Delay (tRRD):",
SI_IDS_MEM_T_RC,"Minimum Active to Auto-Refresh Delay (tRC):",
SI_IDS_MEM_T_RFC,"Minimum Recovery Delay (tRFC):",
SI_IDS_MEM_ECC,"ECC:",
SI_IDS_MEM_T_WR,"Minimum Write Recovery time (tWR):",
SI_IDS_MEM_T_WTR,"Minimum Write to Read CMD Delay (tWTR):",
SI_IDS_MEM_T_RTP,"Minimum Read to Pre-charge CMD Delay (tRTP):",
SI_IDS_MEM_T_FAW,"Minimum Four Activate Window Delay (tFAW):",
SI_IDS_MEM_OPTEMP,"Operating temperature range:",
SI_IDS_MEM_ASR,"Supports Auto Self-Refresh:",
SI_IDS_MEM_PASR,"Supports Partial Array Self-Refresh:",
SI_IDS_MEM_SENSOR,"Thermal Sensor present:",
SI_IDS_MEM_ODTS,"Supports On-Die Thermal Sensor readout:",
SI_IDS_MEM_HEIGHT,"Module Height:",
SI_IDS_MEM_THICKNESS,"Module Thickness:",
SI_IDS_MEM_WIDTH,"Module Width:",
SI_IDS_MEM_T_AC,"Data access time from clock (tAC):",
SI_IDS_MEM_T_IS,"Address/Command Setup Time Before Clock (tIS):",
SI_IDS_MEM_T_IH,"Address/Command Hold Time After Clock (tIH):",
SI_IDS_MEM_T_DS,"Data Input Setup Time Before Strobe (tDS):",
SI_IDS_MEM_T_DH,"Data Input Hold Time After Strobe (tDH):",
SI_IDS_MEM_T_DQSQ,"Maximum DQS to DQ Skew (tDQSQ):",
SI_IDS_MEM_T_QHS,"Maximum Read Data Hold Skew (tQHS):",
SI_IDS_MEM_T_PLL,"PLL Relock Time:",
SI_IDS_MEM_BURST,"Supported Burst Lengths:",
SI_IDS_MEM_REFRESH,"Refresh Rate:",
SI_IDS_MEM_CSLAT,"Supported CS Latencies:",
SI_IDS_MEM_WELAT,"Supported WE Latencies:",
SI_IDS_MEM_CONCAP,"Supports Concurrent Auto Precharge:",
SI_IDS_MEM_FASTAP,"Supports Fast AP:",
SI_IDS_MEM_PRECHALL,"Supports Precharge All:",
SI_IDS_MEM_WRBURST,"Supports Write/Read Burst:",
SI_IDS_MEM_WRTIMES,"Supported Write recovery times:",
SI_IDS_MEM_ALLAT,"Supported Additive Latencies:",
SI_IDS_MEM_TERM,"Supported Terminations",
SI_IDS_MEM_DRIVERS,"Supported drivers:",
SI_IDS_MEM_RANKS,"Number of ranks:",
SI_IDS_MEM_XMPREV,"XMP Revision:",
SI_IDS_MEM_T_REFI,"Maximum tREFI Time (Average Periodic Refresh Interval):",
SI_IDS_MEM_WRCMD,"Write to Read CMD Turn-around Time Optimizations:",
SI_IDS_MEM_RWCMD,"Read to Write CMD Turn-around Time Optimizations:",
SI_IDS_MEM_B2BCMD,"Back 2 Back CMD Turn-around Time Optimizations:",
SI_IDS_MEM_CMDRATE,"System CMD Rate Mode:",
SI_IDS_MEM_EPP_OPTIMAL,"Profile for Optimal Performance:",
SI_IDS_MEM_ADDRDRIVE,"Address Drive Strength:",
SI_IDS_MEM_CSDRIVE,"Chip Select Drive Strength:",
SI_IDS_MEM_CLKDRIVE,"Clock Drive Strength:",
SI_IDS_MEM_DATADRIVE,"Data Drive Strength:",
SI_IDS_MEM_DQSDRIVE,"DQS Drive Strength:",
SI_IDS_MEM_ADDRCMDDELAY,"Address/Command Fine Delay:",
SI_IDS_MEM_ADDRCMDSETUP,"Address/Command Setup Time:",
SI_IDS_MEM_CSDELAY,"Chip Select Delay:",
SI_IDS_MEM_CSSETUP,"Chip Select Setup Time:",
SI_IDS_MEM_NONSTD_TYPE,"Non-standard SDRAM type:",
SI_IDS_MEM_MODULE_TYPE,"Module type:",
SI_IDS_MEM_REF_CARD,"Reference raw card used:",
SI_IDS_MEM_DRAM_MANUF,"DRAM manufacture name:",
SI_IDS_MEM_DRAM_ROWS,"Number of DRAM rows:",
SI_IDS_MEM_DRAM_REGS,"Number of registers:",
SI_IDS_MEM_REG_MANUF,"Register manufacture name:",
SI_IDS_MEM_REG_REV,"Register revision:",
SI_IDS_MEM_REG_TYPE,"Register type:",
SI_IDS_MEM_CMDDRIVE_A,"Command/Address A Outputs Drive Strength:",
SI_IDS_MEM_CMDDRIVE_B,"Command/Address B Outputs Drive Strength:",
SI_IDS_MEM_CTRLDRIVE_A,"Control Signals A Outputs Drive Strength:",
SI_IDS_MEM_CTRLDRIVE_B,"Control Signals B Outputs Drive Strength:",
SI_IDS_MEM_Y1Y3DRIVE,"Y1/Y1# and Y3/Y3# Clock Outputs Drive Strength:",
SI_IDS_MEM_Y0Y2DRIVE,"Y0/Y0# and Y2/Y2# Clock Outputs Drive Strength:",
SI_IDS_MEM_T_CKMAX,"Maximum clock cycle time (tCKmax):",
SI_IDS_MEM_T_RFC2, "Minimum Auto-Refresh to Active/Auto-Refresh Command Period (tRFC2):",
SI_IDS_MEM_T_RFC4, "Minimum Auto-Refresh to Active/Auto-Refresh Command Period (tRFC4):",
SI_IDS_MEM_T_RRD_S,"Minimum Activate to Activate Delay Time (tRRD_Smin), different bank group:",
SI_IDS_MEM_T_RRD_L,"Minimum Activate to Activate Delay Time (tRRD_Lmin), same bank group:",
SI_IDS_MEM_T_CCD_L,"Minimum CAS to CAS Delay Time (tCCD_Lmin), same bank group:",
SI_IDS_MEM_T_MAW,"Maximum Activate Window in units of tREFI (tMAW):",
SI_IDS_MEM_STEPPING,"DRAM Stepping:",
SI_IDS_MEM_PACKAGE,"SDRAM Package Type:",
SI_IDS_MEM_MAC,"Maxium Activate Count (MAC):",
SI_IDS_MEM_PPR,"Post Package Repair supported:",
SI_IDS_MEM_HEAT_SPREAD,"Heat Spreader Solution present:",
SI_IDS_MEM_ODTDRIVE,"ODT Drive Strength:",
SI_IDS_MEM_CKEDRIVE,"CKE Drive Strength:",
SI_IDS_MEM_DATABUF_REV,"Data Buffer revision:",
SI_IDS_MEM_MDQDRIVE_1866,"MQT Drive Strength for data rate <= 1866:",
SI_IDS_MEM_MDQREAD_1866,"MDQ Read Termination Strength for data rate <= 1866:",
SI_IDS_MEM_DRAMDRIVE_1866,"DRAM Drive Strength for data rate <= 1866:",
SI_IDS_MEM_ODTRTT_WR_1866,"DRAM ODT Strength (RTT_WR) for data rate <= 1866:",
SI_IDS_MEM_ODTRTT_NOM_1866,"DRAM ODT Strength (RTT_NOM) for data rate <= 1866:",
SI_IDS_MEM_ODTRTT_PARK_R0R1_1866, "DRAM ODT Strength (RTT_PARK), Package Ranks 0 & 1 for data rate <= 1866:",
SI_IDS_MEM_ODTRTT_PARK_R2R3_1866, "DRAM ODT Strength (RTT_PARK), Package Ranks 2 & 3 for data rate <= 1866:",
SI_IDS_MEM_MDQDRIVE_2400, "MQT Drive Strength for 1866 < data rate <= 2400:",
SI_IDS_MEM_MDQREAD_2400, "MDQ Read Termination Strength for 1866 < data rate <= 2400:",
SI_IDS_MEM_DRAMDRIVE_2400, "DRAM Drive Strength for data rate for 1866 < data rate <= 2400:",
SI_IDS_MEM_ODTRTT_WR_2400, "DRAM ODT Strength (RTT_WR) for 1866 < data rate <= 2400:",
SI_IDS_MEM_ODTRTT_NOM_2400,"DRAM ODT Strength (RTT_NOM) for 1866 < data rate <= 2400:",
SI_IDS_MEM_ODTRTT_PARK_R0R1_2400, "DRAM ODT Strength (RTT_PARK), Package Ranks 0 & 1 for 1866 < data rate <= 2400:",
SI_IDS_MEM_ODTRTT_PARK_R2R3_2400, "DRAM ODT Strength (RTT_PARK), Package Ranks 2 & 3 for 1866 < data rate <= 2400:",
SI_IDS_MEM_MDQDRIVE_3200, "MQT Drive Strength for 2400 < data rate <= 3200:",
SI_IDS_MEM_MDQREAD_3200, "MDQ Read Termination Strength for 2400 < data rate <= 3200",
SI_IDS_MEM_DRAMDRIVE_3200, "DRAM Drive Strength for data rate for 2400 < data rate <= 3200",
SI_IDS_MEM_ODTRTT_WR_3200, "DRAM ODT Strength (RTT_WR) for 2400 < data rate <= 3200",
SI_IDS_MEM_ODTRTT_NOM_3200, "DRAM ODT Strength (RTT_NOM) for 2400 < data rate <= 3200",
SI_IDS_MEM_ODTRTT_PARK_R0R1_3200, "DRAM ODT Strength (RTT_PARK), Package Ranks 0 & 1 for 2400 < data rate <= 3200",
SI_IDS_MEM_ODTRTT_PARK_R2R3_3200, "DRAM ODT Strength (RTT_PARK), Package Ranks 2 & 3 for 2400 < data rate <= 3200",

#
# [Other Mem related]
SI_IDS_MEM_SLOT,"Slot %i:",
SI_IDS_MEM_YEAR_WEEK,"Year: %i, Week: %i",
SI_IDS_MEM_FRONT_BACK,"Front: %i - %i mm, Back: %i - %i mm",
SI_IDS_MEM_EPP_PROFILE_FP,"[EPP Profile FP%i] %s",
SI_IDS_MEM_EPP_PROFILE_AP,"[EPP Profile AP%i] %s",
SI_IDS_MEM_XMP_PROFILE,"[XMP Profile %i] %s",
SI_IDS_MEM_SDRAM,"SDRAM",
SI_IDS_MEM_DDR_SDRAM,"DDR SDRAM",
SI_IDS_MEM_DDR2_SDRAM,"DDR2 SDRAM",
SI_IDS_MEM_DDR2_FB_SDRAM,"DDR2 Fully Buffered SDRAM",
SI_IDS_MEM_DDR2_FB_SDRAM_PROBE,"DDR2 Fully Buffered SDRAM Probe",
SI_IDS_MEM_DDR3_SDRAM,"DDR3 SDRAM",
SI_IDS_MEM_DDR4_SDRAM,"DDR4 SDRAM",
#
SI_CPU_NO_TYPESTRING,"No CPU String",
#
# [SMART Attributes]
SMART_ATTR_UNKNOWN_ATTRIBUTE,"(Unknown attribute)",
SMART_ATTR_INVALID_ID,"Invalid Attribute ID",
SMART_ATTR_RAW_READ_ERROR_RATE,"Raw Read Error Rate",
SMART_ATTR_THROUGHPUT_PERFORMANCE,"Throughput Performance",
SMART_ATTR_SPIN_UP_TIME,"Spin Up Time",
SMART_ATTR_START_STOP_COUNT,"Start/Stop Count",
SMART_ATTR_REALLOCATED_SECTOR_COUNT,"Reallocated Sector Count",
SMART_ATTR_READ_CHANNEL_MARGIN,"Read Channel Margin",
SMART_ATTR_SEEK_ERROR_RATE,"Seek Error Rate",
SMART_ATTR_SEEK_TIME_PERFORMANCE,"Seek Time Performance",
SMART_ATTR_POWER_ON_TIME,"Power On Time",
SMART_ATTR_SPIN_RETRY_COUNT,"Spin Retry Count",
SMART_ATTR_CALIBRATION_RETRY_COUNT,"Calibration Retry Count",
SMART_ATTR_POWER_CYCLE_COUNT,"Power Cycle Count",
SMART_ATTR_SOFT_READ_ERROR_RATE,"Soft Read Error Rate",
SMART_ATTR_AVERAGE_FLYING_HEIGHT_CONTROL,"Average Flying Height control",
SMART_ATTR_MAXIMUM_FLYING_HEIGHT_CONTROL,"Maximum Flying Height control",
SMART_ATTR_TRANSLATION_TABLE_REBUILD,"Translation Table Rebuild",
SMART_ATTR_WEAR_LEVELING_COUNT,"Wear Leveling Count",
SMART_ATTR_UNEXPECTED_POWER_LOSS_COUNT,"Unexpected Power Loss Count",
SMART_ATTR_PROGRAM_FAIL_COUNT_CHIP,"Program Fail Count (Chip)",
SMART_ATTR_ERASE_FAIL_COUNT_CHIP,"Erase Fail Count (Chip)",
SMART_ATTR_USED_RSVD_BLOCK_COUNT_CHIP,"Used Reserved Block Count (Chip)",
SMART_ATTR_USED_RSVD_BLOCK_COUNT_TOTAL,"Used Reserved Block Count (Total)",
SMART_ATTR_UNUSED_RSVD_BLOCK_COUNT_TOTAL,"Unused Reserved Block Count (Total)",
SMART_ATTR_PROGRAM_FAIL_COUNT_TOTAL,"Program Fail Count (Total)",
SMART_ATTR_ERASE_FAIL_COUNT_TOTAL,"Erase Fail Count (Total)",
SMART_ATTR_SATA_DOWNSHIFT_ERROR_COUNT,"SATA Downshift Error Count",
SMART_ATTR_END_TO_END_ERROR,"End-to-End error",
SMART_ATTR_HEAD_STABILITY,"Head Stability",
SMART_ATTR_INDUCED_OP_VIBRATION_DETECTION,"Induced Op-Vibration Detection",
SMART_ATTR_REPORTED_UNCORRECTABLE_ERRORS,"Reported Uncorrectable Errors",
SMART_ATTR_COMMAND_TIMEOUT,"Command Timeout",
SMART_ATTR_HIGH_FLY_WRITES,"High Fly Writes",
SMART_ATTR_TEMP_DIFFERENCE_FROM_100,"Temperature Difference from 100",
SMART_ATTR_G_SENSE_ERROR_RATE,"G-sense Error Rate",
SMART_ATTR_POWER_OFF_RETRACT_COUNT,"Power off Retract Count",
SMART_ATTR_LOAD_CYCLE_COUNT,"Load Cycle Count",
SMART_ATTR_TEMPERATURE,"Temperature",
SMART_ATTR_HARDWARE_ECC_RECOVERED,"Hardware ECC Recovered",
SMART_ATTR_REALLOCATION_EVENT_COUNT,"Reallocation Event Count",
SMART_ATTR_CURRENT_PENDING_SECTOR_COUNT,"Current Pending Sector Count",
SMART_ATTR_UNCORRECTABLE_SECTOR_COUNT,"Uncorrectable Sector Count",
SMART_ATTR_ULTRADMA_CRC_ERROR_COUNT,"UltraDMA CRC Error Count",
SMART_ATTR_WRITE_ERROR_COUNT,"Write Error Count",
SMART_ATTR_OFF_TRACK_ERRORS,"Off Track Errors",
SMART_ATTR_DATA_ADDRESS_MARK_ERRORS,"Data Address Mark Errors",
SMART_ATTR_ERROR_CORRECTION_CODE_ERRORS,"Error Correction Code Errors",
SMART_ATTR_SOFT_ECC_CORRECTION,"Soft ECC Correction",
SMART_ATTR_THERMAL_ASPERITY_RATE,"Thermal Asperity Rate",
SMART_ATTR_FLYING_HEIGHT,"Flying Height",
SMART_ATTR_SPIN_HIGH_CURRENT,"Spin High Current",
SMART_ATTR_SPIN_BUZZ,"Spin Buzz",
SMART_ATTR_OFFLINE_SEEK_PERFORMANCE,"Offline Seek Performance",
SMART_ATTR_VIBRATION_DURING_WRITE,"Vibration During Write",
SMART_ATTR_SHOCK_DURING_WRITE,"Shock During Write",
SMART_ATTR_GROUND_SEEK_ERRORS_RRO_C_ERP,"Ground Seek Errors Count / RRO-C ERP Count",
SMART_ATTR_GROUND_LOAD_ERRORS_COUNT,"Ground Load Errors Count",
SMART_ATTR_GROUND_SPINUP_ERRORS,"Ground Spin-up Errors",
SMART_ATTR_UNEXPECTED_ERRORS_COUNT,"Unexpected Errors Count",
SMART_ATTR_UNLOCK_MISREAD_COUNT,"Unlock/Misread Count",
SMART_ATTR_FLASHROM_ECC_CORRECTED_COUNT,"FlashROM ECC Corrected Count",

SMART_ATTR_DISK_SHIFT,"Disk shift",
SMART_ATTR_LOADED_HOURS,"Loaded hours",
SMART_ATTR_LOAD_UNLOAD_RETRY_COUNT,"Load/Unload retry count",
SMART_ATTR_LOAD_FRICTION,"Load friction",
SMART_ATTR_LOAD_IN_TIME,"Load-in Time",
SMART_ATTR_TORQUE_AMPLIFICATION_COUNT,"Torque Amplification Count",
SMART_ATTR_GMR_HEAD_AMPLITUDE,"GMR Head Amplitude",
SMART_ATTR_ENDURANCE_REMAINING,"Endurance Remaining",

SMART_ATTR_HEAD_FLYING_HOURS,"Head flying hours",
SMART_ATTR_TOTAL_LBAS_WRITTEN,"Total LBAs Written",
SMART_ATTR_TOTAL_LBAS_READ,"Total LBAs Read",
SMART_ATTR_READ_ERROR_RETRY_RATE,"Read Error Retry Rate",
SMART_ATTR_FREE_FALL_PROTECTION,"Free Fall Protection",

# [SMART Attributes SSD - Indilinx]
SMART_ATTR_INITIAL_BAD_BLOCK_COUNT,"Initial Bad Block Count",
SMART_ATTR_AVAILABLE_OP_BLOCK_COUNT, "Available OP Block Count",
SMART_ATTR_PROGRAM_FAILURE_BLOCK_COUNT,"Program Failure Block Count",
SMART_ATTR_ERASE_FAILURE_BLOCK_COUNT,"Erase Failure Block Count",
SMART_ATTR_READ_FAILURE_BLOCK_COUNT,"Read Failure Block Count (Uncorrectable)",
SMART_ATTR_HOST_READS_GB,"Host reads (GB)",
SMART_ATTR_HOST_WRITES_GB,"Host writes (GB)",
SMART_ATTR_READ_FAILURE_BLOCK_COUNT_UNCORRECTABLE,"Total Count of Read Sectors",
SMART_ATTR_TOTAL_COUNT_OF_READ_SECTORS,"Total Count of Read Sectors",
SMART_ATTR_TOTAL_COUNT_OF_WRITE_SECTORS,"Total Count of Write Sectors",
SMART_ATTR_TOTAL_COUNT_OF_READ_COMMANDS,"Total Count of Read Commands",
SMART_ATTR_TOTAL_COUNT_OF_WRITE_COMMANDS,"Total Count of Write Commands",
SMART_ATTR_TOTAL_COUNT_OF_ERROR_BITS_FROM_FLASH,"Total Count of Error Bits from Flash",
SMART_ATTR_TOTAL_COUNT_OF_READ_SECTORS_W_CORRECTABLE_ERRORS,"Total Count of Read Sectors with Correctable Errors",
SMART_ATTR_BAD_BLOCK_FULL_FLAG,"Bad Block Full Flag",
SMART_ATTR_MAXIMUM_PE_COUNT_SPECIFICATION,"Maximum PE Count Specification",
SMART_ATTR_MINIMUM_ERASE_COUNT,"Minimum Erase Count",
SMART_ATTR_MAXIMUM_ERASE_COUNT,"Maximum Erase Count",
SMART_ATTR_AVERAGE_ERASE_COUNT,"Average Erase Count",
SMART_ATTR_REMAINING_LIFE,"Remaining Life (%)",
SMART_ATTR_INDILINX_INTERNAL,"Indilinx Internal",
SMART_ATTR_SATA_ERROR_COUNT_CRC,"SATA Error Count CRC",
SMART_ATTR_SATA_ERROR_COUNT_HANDSHAKE,"SATA Error Count Handshake",
SMART_ATTR_LIFETIME_REMAINING,"Lifetime Remaining",
SMART_ATTR_TOTAL_NAND_PROG_COUNT_GB,"Total NAND programming count (GB)",


# [SMART Attributes SSD - OCZ/Corsair]
SMART_ATTR_RETIRED_BLOCK_COUNT,"Retired Block Count",
SMART_ATTR_PROGRAM_ERASE_CYCLES,"Program/Erase Cycles",
SMART_ATTR_RESERVED_BLOCK_COUNT,"Reserved Block Count",
SMART_ATTR_PROGRAM_FAIL_BLOCK_COUNT,"Program Fail Block Count",
SMART_ATTR_ERASE_FAIL_BLOCK_COUNT,"Erase Fail Block Count",
SMART_ATTR_UNEXPECTED_POWER_LOSS_COUNT,"Unexpected Power Loss Count",
SMART_ATTR_WEAR_RANGE_DELTA,"Wear Range Delta",
SMART_ATTR_ERASE_FAIL_COUNT,"Erase Fail Count",
SMART_ATTR_ON_THE_FLY_ECC_UNCORRECTABLE_ERROR_COUNT,"On the fly ECC Uncorrectable Error Count",
SMART_ATTR_UNCORRECTABLE_SOFT_READ_ERROR_RATE,"Uncorrectable Soft Read Error Rate",
SMART_ATTR_LIFE_CURVE_STATUS,"Life Curve Status",
SMART_ATTR_SSD_LIFE_LEFT,"SSD Life Left",
SMART_ATTR_AVAILABLE_RESERVED_SPACE,"Available Reserved Space",
SMART_ATTR_SANDFORCE_INTERNAL,"SandForce Internal",
SMART_ATTR_POWER_FAIL_BACKUP_HEALTH,"Power Fail Backup Health",
SMART_ATTR_LIFETIME_WRITES_FROM_HOST,"Lifetime Writes from Host",
SMART_ATTR_LIFETIME_READS_FROM_HOST,"Lifetime Reads from Host",

# [SMART Attributes SSD - Intel]
SMART_ATTR_PROGRAM_FAIL_COUNT,"Program Fail Count",
SMART_ATTR_POWER_LOSS_PROTECTION_FAILURE,"Power Loss Protection Failure",
SMART_ATTR_CASE_TEMP_DIFFERENCE_FROM_100,"Case Temperature (Difference from 100)",
SMART_ATTR_UNSAFE_SHUTDOWN_COUNT,"Unsafe Shutdown Count",
SMART_ATTR_HOST_WRITES,"Host Writes",
SMART_ATTR_TIMED_WORKLOAD_MEDIA_WEAR_INDICATOR,"Timed Workload Media Wear Indicator",
SMART_ATTR_TIMED_WORKLOAD_HOST_READS_PERCENTAGE,"Timed Workload Host Reads Percentage",
SMART_ATTR_WORKLOAD_TIMER,"Workload Timer",
SMART_ATTR_MEDIA_WEAROUT_INDICATOR,"Media Wearout Indicator",
SMART_ATTR_NAND_WRITES,"Total NAND Writes (GB)",

# [SMART Attributes SSD - Samsung]
SMART_ATTR_RUNTIME_BAD_BLOCK_TOTAL,"Runtime bad block (Total)",
SMART_ATTR_AIR_FLOW_TEMPERATURE,"Air Flow temperature",
SMART_ATTR_ECC_ERROR_RATE,"ECC Error Rate",
SMART_ATTR_SUPERCAP_STATUS,"Supercap Status",
SMART_ATTR_EXCEPTION_MODE_STATUS,"Exception Mode Status",
SMART_ATTR_POWER_RECOVERY_COUNT,"Power Recovery Count",

# [SMART Attributes SSD - Micron]
SMART_ATTR_NEW_FAILING_BLOCK_COUNT,"New Failing Block Count",
SMART_ATTR_BLOCK_WEAR_LEVELING_COUNT_AVERAGE_BLOCK_ERASE_COUNT,"Block Wear Leveling Count / Average Block Erase Count",
SMART_ATTR_UNEXPECTED_POWER_LOST_COUNT,"Unexpected Power Loss Count",
SMART_ATTR_NON_4K_ALIGNED_ACCESS_COUNT,"Non-4K Aligned Access Count",
SMART_ATTR_ERROR_CORRECTION_COUNT,"Error Correction Count",
SMART_ATTR_CUMULATIVE_CORRECTED_ECC,"Cumulative Corrected ECC",
SMART_ATTR_FACTORY_BAD_BLOCK_COUNT,"Factory Bad Block Count",
SMART_ATTR_PERCENTAGE_LIFETIME_REMAINING,"Percentage Lifetime Remaining",
SMART_ATTR_PERCENTAGE_LIFETIME_USED,"Percentage Lifetime Used",
SMART_ATTR_WRITE_ERROR_RATE,"Write Error Rate",
SMART_ATTR_SUCCESSFUL_RAIN_RECOVERY_COUNT,"Successful RAIN Recovery Count",
SMART_ATTR_TOTAL_HOST_SECTOR_WRITES,"Total Host Sector Writes",
SMART_ATTR_HOST_PROGRAM_PAGE_COUNT,"Host Program Page Count",
SMART_ATTR_BACKGROUND_PROGRAM_PAGE_COUNT,"Background Program Page Count",


# [SMART Attributes SSD - Kingston]
SMART_ATTR_SATA_PHY_ERROR_COUNT,"SATA PHY Error Count",
SMART_ATTR_BAD_BLOCK_COUNT,"Bad Block Count",
SMART_ATTR_ERASE_COUNT,"Erase Count",
SMART_ATTR_BAD_CLUSTER_TABLE_COUNT,"Bad Cluster Table Count",
SMART_ATTR_HALT_SYSTEM_FLASH_ID,"Halt System, Flash ID",
SMART_ATTR_FIRMWARE_VERSION_INFORMATION,"Firmware Version Information",
SMART_ATTR_ECC_FAIL_RECORD,"ECC Fail Record",
SMART_ATTR_AVERAGE_ERASE_COUNT_MAX_ERASE_COUNT,"Average Erase Count, Max Erase Count",
SMART_ATTR_GOOD_BLOCK_COUNT_SYSTEM_BLOCK_COUNT,"Good Block Count, System Block Count",
SMART_ATTR_WRITE_HEAD,"Write Head",

# [SMART Export Report]
SMART_RPTHDR_TIME_OF_EXPORT,"Time of export:",
SMART_RPTHDR_DEVICE_INFO,"Device information:",
SMART_RPTHDR_DEVICE_ID,"Device ID:",
SMART_RPTHDR_INTERFACE,"Interface:",
SMART_RPTHDR_DEVICE_CAPACITY,"Device Capacity:",
SMART_RPTHDR_SERIAL_NO,"Serial Number:",
SMART_RPTHDR_MODEL_NO,"Model Number:",
SMART_RPTHDR_FIRMWARE_REVISION,"Firmware Revision:",
SMART_RPTHDR_PARTITIONS,"Partitions:",
SMART_RPTHDR_ATA_INFO,"ATA information:",
SMART_RPTHDR_DISK_GEOMETRY,"Disk geometry:",
SMART_RPTHDR_CYLINDERS,"Cylinders:",
SMART_RPTHDR_TRACKS_PER_CYLINDER,"Tracks/Cylinder:",
SMART_RPTHDR_SECTORS_PER_TRACK,"Sectors/Track:",
SMART_RPTHDR_BYTES_PER_SECTOR,"Bytes/Sector:",
SMART_RPTHDR_TOTAL_DISK_SECTORS,"Total disk sectors:",
SMART_RPTHDR_LOGICAL_SECTOR_SIZE,"Logical sector size:",
SMART_RPTHDR_PHYSICAL_SECTOR_SIZE,"Physical sector size:",
SMART_RPTHDR_MEDIA_ROTATION_RATE,"Media rotation rate:",
SMART_RPTHDR_BUFFER_SIZE,"Buffer size:",
SMART_RPTHDR_ECC_SIZE,"ECC size:",
SMART_RPTHDR_STANDARDS_COMPLIANCE,"Standards compliance:",
SMART_RPTHDR_ATA8_ACS_SUPPORTED,"ATA8-ACS Supported:",
SMART_RPTHDR_ATA_ATAPI_7_SUPPORTED,"ATA/ATAPI-7 Supported:",
SMART_RPTHDR_ATA_ATAPI_6_SUPPORTED,"ATA/ATAPI-6 Supported:",
SMART_RPTHDR_ATA_ATAPI_5_SUPPORTED,"ATA/ATAPI-5 Supported:",
SMART_RPTHDR_ATA_ATAPI_4_SUPPORTED,"ATA/ATAPI-4 Supported:",
SMART_RPTHDR_SERIAL_PARALLEL,"Serial/Parallel:",
SMART_RPTHDR_SATA3_COMPLIANCE,"SATA 3.0 Compilance:",
SMART_RPTHDR_SATA2_6_COMPLIANCE,"SATA 2.6 Compilance:",
SMART_RPTHDR_SATA2_5_COMPLIANCE,"SATA 2.5 Compilance:",
SMART_RPTHDR_SATAII_COMPLIANCE,"SATA II: Ext Compilance:",
SMART_RPTHDR_SATA1_0_A_COMPLIANCE,"SATA 1.0a Compilance:",
SMART_RPTHDR_ATA8_AST_COMPLIANCE,"ATA8-AST Compilance:",
SMART_RPTHDR_ATA_ATAPI7_COMPLIANCE,"ATA/ATAPI-7 Compilance:",
SMART_RPTHDR_ATA8_APT_COMPLIANCE,"ATA8-APT Compliance:",
SMART_RPTHDR_WORLD_WIDE_ID,"World Wide ID:",
SMART_RPTHDR_FEATURE_SUPPORT,"Feature support:",
SMART_RPTHDR_SMART_SUPPORTED,"SMART supported:",
SMART_RPTHDR_SMART_ENABLED,"SMART enabled:",
SMART_RPTHDR_SELF_TEST_SUPPORTED,"SMART self-test supported:",
SMART_RPTHDR_ERROR_LOG_SUPPORTED,"SMART error log supported:",
SMART_RPTHDR_LBA_SUPPORTED,"LBA supported:",
SMART_RPTHDR_IORDY_SUPPORTED,"IORDY supported:",
SMART_RPTHDR_CFAST_SUPPORTED,"CFast supported:",
SMART_RPTHDR_DMA_SUPPORTED,"DMA supported:",
SMART_RPTHDR_MAX_MULTIWORD_DMA_MODE_SUPPORTED,"Maximum Multiword DMA mode supported:",
SMART_RPTHDR_MULTIWORD_DMA_SELECTED,"Multiword DMA selected:",
SMART_RPTHDR_MAX_ULTRADMA_MODE_SUPPORTED,"Maximum UltraDMA mode supported:",
SMART_RPTHDR_ULTRADMA_SELECTED,"UltraDMA selected:",
SMART_RPTHDR_MAX_PIO_MODE_SUPPORTED,"Maximum PIO mode supported:",
SMART_RPTHDR_SATA_COMPLIANCE,"SATA Compliance:",
SMART_RPTHDR_NCQ_PRIORITY_INFO_SUPPORTED,"NCQ priority information supported:",
SMART_RPTHDR_NCQ_COMMANDS_OUTSTAND_SUPPORTED,"Unload while NCQ commands are outstanding supported:",
SMART_RPTHDR_PHY_EVENT_COUNTERS_SUPPORTED,"Phy Event Counters supported:",
SMART_RPTHDR_RECEIPT_POWER_MANAGEMENT_REQUESTS_SUPPORTED,"Receipt of power management requests supported:",
SMART_RPTHDR_NCQ_FEATURE_SET_SUPPORTED,"NCQ feature set supported:",
SMART_RPTHDR_SATA_GEN2_SIGNALING_SUPPORTED,"SATA Gen2 Signaling Speed (3.0Gb/s) supported:",
SMART_RPTHDR_SATA_GEN1_SIGNALING_SUPPORTED,"SATA Gen1 Signaling Speed (1.5Gb/s) supported:",
SMART_RPTHDR_SOFTWARE_SETTINGS_PRESERVATION,"Software Settings Preservation:",
SMART_RPTHDR_IN_ORDER_DATA_DELIVERY,"In-order data delivery:",
SMART_RPTHDR_INITIATING_POWER_MANAGEMENT,"Initiating power management:",
SMART_RPTHDR_DMA_SETUP_AUTO_ACTIVATION,"DMA Setup auto-activation:",
SMART_RPTHDR_NON_ZERO_BUFFER_OFFSETS,"Non-zero buffer offsets:",
SMART_RPTHDR_TRUSTED_COMPUTING_SUPPORTED,"Trusted Computing supported:",
SMART_RPTHDR_HPA_SUPPORTED,"Host Protected Area (HPA) supported:",
SMART_RPTHDR_READ_LOOK_AHEAD_SUPPORTED,"Read look-ahead supported:",
SMART_RPTHDR_READ_LOOK_AHEAD_ENABLED,"Read look-ahead enabled:",
SMART_RPTHDR_WRITE_CACHE_SUPPORTED,"Write cache supported:",
SMART_RPTHDR_WRITE_CACHE_ENABLED,"Write cache enabled:",
SMART_RPTHDR_POWER_MANAGEMENT_SUPPORTED,"Power management supported:",
SMART_RPTHDR_SECURITY_MODE_SUPPORTED,"Security mode supported:",
SMART_RPTHDR_SECURITY_MODE_ENABLED,"Security mode enabled:",
SMART_RPTHDR_DCO_SUPPORTED,"Device Configuration Overlay (DCO) supported:",
SMART_RPTHDR_48BIT_ADDRESS_SUPPORTED,"48bit Addressing supported:",
SMART_RPTHDR_AAM_SUPPORTED,"Auto Acoustic Managment (AAM) supported:",
SMART_RPTHDR_AAM_ENABLED,"Auto Acoustic Managment (AAM) enabled:",
SMART_RPTHDR_RECOMMENDED_AAM_LEVEL,"Recommended AAM level:",
SMART_LEVEL_VENDOR_SPECIFIC,"Vendor specific",
SMART_LEVEL_MIN_ACOUSTIC_EMANATION_LEVEL,"Minimum acoustic emanation level",
SMART_LEVEL_INT_ACOUSTIC_MANAGEMENT_LEVELS,"Intermediate acoustic management levels",
SMART_LEVEL_MAX_PERFORMANCE,"Maximum performance",
SMART_RPTHDR_CURRENT_AAM_LEVEL,"Current AAM level:",
SMART_RPTHDR_PUIS_SUPPORTED,"Power-up in Standby (PUIS) supported:",
SMART_RPTHDR_PUIS_ENABLED,"Power-up in Standby (PUIS) enabled:",
SMART_RPTHDR_APM_SUPPORTED,"Advanced Power Management (APM) supported:",
SMART_RPTHDR_APM_ENABLED,"Advanced Power Management (APM) enabled:",
SMART_RPTHDR_CURRENT_APM_LEVEL,"Current APM level:",
SMART_LEVEL_MIN_POWER_STANDBY,"Minimum power consumption with Standby",
SMART_LEVEL_INT_POWER_STANDBY,"Intermediate power management levels with Standby",
SMART_LEVEL_MIN_POWER_WO_STANDBY,"Minimum power consumption without Standby",
SMART_LEVEL_INT_POWER_WO_STANDBY,"Intermediate power management levels without Standby",
SMART_RPTHDR_CFA_SUPPORTED,"CompactFlash Association (CFA) supported:",
SMART_RPTHDR_GPL_SUPPORTED,"General Purpose Logging (GPL) supported:",
SMART_RPTHDR_STREAMING_SUPPORTED,"Streaming supported:",
SMART_RPTHDR_MEDIA_CARD_PASS_THROUGH_SUPPORTED,"Media card pass through supported:",
SMART_RPTHDR_MEDIA_CARD_PASS_THROUGH_ENABLED,"Media card pass through enabled:",
SMART_RPTHDR_EXTENDED_POWER_SUPPORTED,"Extended power conditions supported:",
SMART_RPTHDR_EXTENDED_POWER_ENABLED,"Extended power conditions enabled:",
SMART_RPTHDR_EXTENDED_STATUS_REPORT_SUPPORTED,"Extended status reporting supported:",
SMART_RPTHDR_EXTENDED_STATUS_REPORT_ENABLED,"Extended status reporting enabled:",
SMART_RPTHDR_WRITE_READ_VERIFY_SUPPORTED,"Write-read-verify supported:",
SMART_RPTHDR_WRITE_READ_VERIFY_ENABLED,"Write-read-verify enabled:",
SMART_RPTHDR_FREE_FALL_SUPPORTED,"Free-fall control supported:",
SMART_RPTHDR_FREE_FALL_ENABLED,"Free-fall control enabled:",
SMART_RPTHDR_TRIM_SUPPORTED,"TRIM command supported:",
SMART_RPTHDR_SCT_SUPPORTED,"SCT command transport supported:",
SMART_RPTHDR_NV_CACHE_ENABLED,"NV Cache enabled:",
SMART_RPTHDR_NV_CACHE_POWER_MAN_SUPPORTED,"NV Cache Power Management supported:",
SMART_RPTHDR_NV_CACHE_POWER_MAN_ENABLED,"NV Cache Power Management enabled:",
SMART_RPTHDR_SMART_HISTORY,"SMART HISTORY:",
