;2013-04-07
IMGVER	0.6
IMGTYPE	1	; I211 with APM

;====================================================================================
;		I N T E L   P R O P R I E T A R Y
;COPYRIGHT (c) 1998 - 2012 BY INTEL CORPORATION.  ALL RIGHTS RESERVED.
;NO PART OF THIS PROGRAM OR PUBLICATION MAY BE REPRODUCED, TRANSMITTED, TRANSCRIBED,
;STORED IN A RETRIEVAL SYSTEM, OR TRANSLATED INTO ANY LANGUAGE OR COMPUTER LANGUAGE
;IN ANY FORM OR BY ANY MEANS, ELECTRONIC, MECHANICAL, MAGNETIC, OPTICAL, CHEMICAL,
;MANUAL, OR OTHERWISE, WITHOUT THE PRIOR WRITTEN PERMISSION OF:
;INTEL CORPORATION
;2200 MISSION COLLEGE BOULEVARD
;SANTA CLARA, CALIFORNIA 95052-8119

;Autoload commands configuration file for I211.

;SYNTAX:
;=======
; The following entries are allowed in file:

; 	Single command record entry:
;	============================
; 		<Record type> <Address> = <Data> <Reset type> <Comment>

;	Series of commands which must be applied in exact sequance
;	===========================================================
;		Ordered_Section_Start

;		<Single record entry #1>
;		.
;		.
;		<Single record entry #N>

;		Ordered_Section_End

;     	Pure comment line like the one you are looking at :-).
;	======================================================

;	Empty line with white characters only.
;	======================================================

; where:
;	<Record type> 	- record type:
;		WALD 	- autoload word record
;		CSRALD 	- CSR autoload record
;		PHYALD 	- PHY autoload record

;	<Address> - address in hexadecimal format from range: 
;		0x00 	- 0x2E 					in WALD records definition
;		0x00000 - 0x1FFFC (4 bytes alignment required)	in CSRALD records definition
;		0x00 	- 0x1F 					in PHYALD records definition

;	<Data>  - Data to set in hexadecimal format:
;		0x0000 		- 0xFFFF 	in WALD and PHYALD records definition
;		0x00000000 	- 0xFFFFFFFF 	in CSRALD records definition

;	<Reset type> - describes set of reset events for which particular record data setting is to be applied:
;		LPG_RST  - LanPower Good Reset only
;		PCIE_RST - PCIe asserted reset and all above
;		SW_RST   - Host software asserted device reset and all above

;	<Comment> - any sequence of printable characters (including space and tab) starting with ';'


;	Duplicates (records with the same value of fields: <Record type> <Address> and <Reset type>) shouldn't 
;	   be defined outside ordered section. If both are found outside ordered section then all but the first found
;	   will be silently ignored by the commands parser. If one of them is defined in ordered section then its counterpart 
;	   outside ordered section will be ignored as well.
	 

	CSRALD 	0x5ba0 	= 0x00001541 	LPG_RST 	; [Intel] Set GPAR_EN from CSR auto config.
	CSRALD 	0x0E34 	= 0x0B403C21	LPG_RST 	; [Intel] Clear EE_SU.LPI_Clock_Stop.

	WALD   	0x0a    = 0x402F     	PCIE_RST	; [Intel] Set GPAR_EN.
	WALD 	0x1b 	= 0x3400 	PCIE_RST        ; [Intel] Default settings.
	WALD 	0x29 	= 0x003C 	PCIE_RST        ; [Intel] Set Wake_pin_enable
	WALD 	0x0d 	= 0x1539 	PCIE_RST	; [Intel] I211 Device ID
	WALD 	0x21 	= 0x0584 	PCIE_RST	; [Intel] Default settings.
	WALD 	0x24 	= 0x0680 	PCIE_RST	; [Intel] Set APM
	WALD 	0x0F 	= 0xF343 	SW_RST 		; [Intel] Set APMPME and TX_LPI_EN.

; Common Customer Configurations
; ==============================
;   Subsystem Vendor ID and Subsystem ID - Uncomment the following lines and insert the values.
;	WALD	0x0B	= 0x0000	PCIE_RST	; Subsystem ID
;	WALD	0x0C	= 0x8086	PCIE_RST	; Susbsystem Vendor ID
;
;   Disable IO BAR - Uncomment the following line.
;	WALD	0x19	= 0x3000	PCIE_RST	; Clear IO_Sup
;
;   Non-default LED Configuration - Uncomment the following lines and set the values for the LED configuration.
;	WALD	0x1C	= 0x0784	PCIE_RST	; LED1 Config
;	WALD	0x1F	= 0x0706	PCIE_RST	; LED0,2 Config
;
;   Enable Power-Down Modes - Uncomment the 1st line to enable power down with the DEV_OFF_N pin.
;			      Uncomment the 2nd line to enable the dynamic power down mode.
;			      Enabling both power down modes is not permitted.
;	WALD	0x1E	= 0xB200	PCIE_RST	; Enable DEV_OFF Power Down
;	WALD	0x1E	= 0x7200	PCIE_RST	; Power Down Settings
;
;   LAN Power Consumption - Uncomment the following line and insert power data to be provided in the PCIe config space.
;	WALD	0x22	= 0x0000	PCIE_RST	; LAN Power Consumption
;
;   Watchdog Configuration - Uncomment the following line to enable the watchdog after reset.
;	WALD	0x2E	= 0x9000	SW_RST		; Enable watchdog
;


Ordered_Section_Start
	CSRALD 	0x5B44 	= 0x00FF00A8 	LPG_RST 	; [Intel] Set NFTS to 0xA8.
	CSRALD 	0x5B40 	= 0x5E000090 	LPG_RST 	; [Intel]  cont.
Ordered_Section_End



